For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Drain the coolant. Refer to Cooling System Draining and Filling .
3. Pull the stem out of the radiator body.
4. Clean or replace the seal and the stem as necessary.

### Installation Procedure

1. Install the stem to the radiator body.
2. Fill the cooling system. Refer to Cooling System Draining and Filling .
3. Lower the vehicle.