For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the passenger front seat. Refer to Bucket Seat Replacement in Seats.
3. Remove the passenger seat adjuster track cover (1). Refer to Front Seat Adjuster Track Finish Cover Replacement in Seats.
4. Remove the nut from the passenger seat belt pretensioner (1).
5. Route the passenger seat belt pretensioner wiring harness (2) through the passenger seat bottom frame.
6. Remove the passenger seat belt pretensioner (1) from the passenger seat bottom frame.
7. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Pretensioner Handling, Shipping, and Scrapping .

### Installation Procedure

1. Install the passenger seat belt pretensioner (1) to the passenger seat bottom frame.
2. Route the passenger seat belt pretensioner wiring harness (2) through the passenger seat bottom frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the nut to the passenger seat belt pretensioner (1).

Tighten
Tighten the nut to 35 N·m (26 lb ft).

4. Install the passenger front seat adjuster track cover (1). Refer to Front Seat Adjuster Track Finish Cover Replacement in Seats.
5. Install the passenger front seat. Refer to Bucket Seat Replacement in Seats.
6. Enable the SIR system. Refer to Enabling the SIR System .