For 1990-2009 cars

### Removal Procedure

The air pump relay is mounted in the right front corner of the engine compartment, near the right turn signal pigtail.

1. Turn OFF the ignition.
2. Disconnect the wiring connector from the air pump relay.
3. Remove the air pump relay from the vehicle.

### Installation Procedure

1. Install the air pump relay into the vehicle.
2. Reconnect the wiring connector to the air pump relay.