For 1990-2009 cars

## Exhaust Heat Shield Replacement Catalytic Converter

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the three-way catalytic converter. Refer to Catalytic Converter Replacement .
3. Remove the rivets at the catalytic converter heat shield.
4. Remove the catalytic converter heat shield from the vehicle.

### Installation Procedure

1. Install the catalytic converter heat shield to the vehicle with rivets.
2. Install the three-way catalytic converter. Refer to Catalytic Converter Replacement .
3. Lower the vehicle.

## Exhaust Heat Shield Replacement Exhaust Muffler

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the exhaust system. Refer to Exhaust System Replacement .
3. Remove the rivets at the exhaust muffler heat shield.
4. Remove the exhaust muffler heat shield from the vehicle.

### Installation Procedure

1. Install the exhaust muffler heat shield to the vehicle with rivets.
2. Install the exhaust system. Refer to Exhaust System Replacement .
3. Lower the vehicle.