For 1990-2009 cars

Usage | Fluid/Lubricant
--- | ---
Automatic Transmission | DEXRON®-III, Automatic Transmission Fluid
Engine Coolant | 50/50 mixture of clean, drinkable water and use only GM Goodwrench® DEX-COOL® or Havoline® DEX-COOL® Coolant
Engine Oil | Engine oil with the American Petroleum Institute Certified For Gasoline Engines Starburst symbol of the proper viscosity Refer to Explanation of Scheduled Services
Hood and Door Hinges | Multi-Purpose Lubricant, Superlube® (GM P/N 12346241 or equivalent)
Hood Latch Assembly, Secondary Latch, Pivots, Spring Anchor and Release Pawl | Lubriplate® Lubricant Aerosol (GM P/N 12346293 or equivalent) or lubricant meeting requirements of NLGI # 2, Category LB or GC-LB
Hydraulic Brake System | Delco Supreme 11® Brake Fluid (GM P/N 12377967 or equivalent DOT-3 Brake Fluid)
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube® (GM P/N 12346241 or equivalent)
Parking Brake Cable Guides | Chassis Lubricant (GM P/N 12377985 or equivalent) or Lubricant meeting requirements of NLGI # 2, Category LB or GC-LB
Power Steering System | GM Power Steering Fluid (GM P/N 1052884 - 1 pint, 1050017 - 1 quart, or equivalent)
Rear Folding Seat, Fuel Door Hinge, Liftgate Hinges, Power Sliding Door Cable | Multi-Purpose Lubricant, Superlube® (GM P/N 12346241 or equivalent)
Sliding Door Track | Lubriplate® Lubricant Aerosol (GM P/N 12346293 or equivalent) or lubricant meeting requirements of NLGI # 2, Category LB or GC-LB
Weatherstrips | Dielectric Silicone Grease (GM P/N 12345579 or equivalent)
Windshield Washer Solvent | GM Optikleen® Washer Solvent (GM P/N 1051515) or equivalent