For 1990-2009 cars

Table 1: | AIR Pump Relay
Table 2: | Cigar Lighter Connector
Table 3: | Starter Relay
Table 4: | Auxiliary Power Outlet-Front
Table 5: | Auxiliary Power Outlet-Rear
Table 6: | Junction Block C1 Underhood
Table 7: | Junction Block C2 Underhood
Table 8: | Junction Block C3 Underhood
Table 9: | Junction Block C4 Underhood
Table 10: | Junction Block C5 Underhood
Table 11: | Junction Block C6 Underhood
Table 12: | Relay Block (Domestic)
Table 13: | Relay Block (Export)

#### AIR Pump Relay

Connector Part Information |

• | 12129716

• | 4 F Metri-pack 280 FLX LK (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | ORN | 3040 | Fused Output
85 | BLK | 339 | Fused Output Ignition 1
86 | BRN | 436 | AIR Injection Reaction Pump Motor Relay Output - Coil
87 | RED | 78 | AIR Injection Reaction Pump Motor Feed

#### Cigar Lighter Connector

Connector Part Information |

• | 12176836

• | 3-Way F Metri-pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 440 | Fused Ignition Feed
B | -- | -- | Not Used
C | BLK | 150 | Ground

#### Starter Relay

Connector Part Information |

• | 12110539

• | 5 F Metri-pack 280 FLX LK (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 402 | Fused Output
85 | ORN/BLK | 1786 | Transmission Park/Neutral Signal
86 | YEL/BLK | 625 | Starter Enable Relay Output - Coil
87 | PPL | 6 | Starter Solenoid Feed
87A | -- | -- | Not Used

#### Auxiliary Power Outlet-Front

Connector Part Information |

• | 12176836

• | 3-Way F Metri-pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 440 | Fused Ignition Feed
B | -- | -- | Not Used
C | BLK | 150 | Ground

#### Auxiliary Power Outlet-Rear

Connector Part Information |

• | 12033934

• | 2-Way F 56 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 2540 | Fused Ignition Feed
B | BLK | 850 | Ground

#### Junction Block C1 Underhood

Connector Part Information |

• | 15303513

• | 68-Way F Metri-pack 280 Series Flexlock (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A4 | -- | -- | Not Used
A5 | DK GRN/WHT | 465 | Fuel Pump Relay Feed-Coil
A6-A7 | -- | -- | Not Used
A8 | ORN | 840 | Fused Battery Feed
A9 | PNK | 339 | Fused Ignition 1 Feed
A10 | WHT | 504 | Engine Coolant Fan 1 (RH) Motor Feed
A11 | -- | -- | Not Used
A12 | PNK | 639 | Fused Ignition 1 Feed
B1-B2 | -- | -- | Not Used
B3 | PNK | 339 | Ignition 1 Fused Output
B4 | RED | 490 | Fuel Pump Relay Feed-N.C. Contact-Prime
B5 | BLK/WHT | 451 | PCM Ground
B6 | -- | -- | Not Used
B7 | PNK | 1339 | Fused Ignition 1 Feed
B8 | -- | -- | Not Used
B9 | PNK | 339 | Fused Ignition 1 Feed
B10-B12 | -- | -- | Not Used
C1 - C8 | -- | -- | Not Used
C9 | PNK | 339 | Fused Ignition 1 Feed
C10 | DK BLU | 473 | Engine Coolant Fan 2 (LH) Relay Output-Coil
C11 | BLK | 1050 | Ground
C12 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3 | BRN | 436 | Air Injection Pump Motor Relay Coil Output
D4-D8 | -- | -- | Not Used
D9 | PNK | 339 | Fused Ignition 1 Feed
D10 | -- | -- | Not Used
D11 | PNK | 439 | Fused Ignition 1 Feed
D12 | TAN/BLK | 231/231 | Oil Pressure Switch Signal
E1 | -- | -- | Not Used
E2 | ORN | 540 | Fused Battery Feed
E3 | -- | -- | Not Used
E4 | LT GRN | 275 | Transaxle Range Switch Feed-PARK
E5 | DK GRN | 389 | Vehicle Speed Signal
E6-E11 | -- | -- | Not Used
E12 | ORN | 2740 | Battery Fused Output
F1 | -- | -- | Not Used
F2 | GRY | 532 | Engine Coolant Fan 1 (RH) Motor Output
F3 | DK GRN | 335 | Coolant Fan 1 Relay Output-Coil
F4 | -- | -- | Not Used
F5 | LT GRN | 24 | Back Up Lamp Feed
F6 | WHT | 17 | Stoplamp Switch Output
F7 | DK GRN/WHT | 459 | A/C CLU Relay Output Coil
F8 | DK GRN | 59 | A/C Compressor Clutch Coil Solenoid Feed
F9 | PNK | 239 | Fused Ignition 1 Feed
F10 | -- | -- | Not Used
F11 | LT BLU | 409 | Engine Coolant Fan 2 (LH) Feed
F12 | -- | -- | Not Used

#### Junction Block C2 Underhood

Connector Part Information |

• | 15303514

• | 68-Way F Metri-pack 280 Series Flexlock (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A4 | -- | -- | Not Used
A5 | LT GRN/BLK | 24 | Backup Lamp-Feed
A6 | WHT | 17 | Stoplamp Switch Output
A7-B4 | -- | -- | Not Used
B5 | GRY | 120 | Fuel Pump Motor Feed
B6-C3 | -- | -- | Not Used
C4 | LT GRN | 275 | Transaxle Range Switch Feed-PARK
C5 | -- | -- | Not Used
C8 | DK GRN | 389 | Vehicle Speed Signal
C9 | -- | -- | Not Used
C10 | PNK | 439 | Fused Ignition 1 Feed
C11-C12 | -- | -- | Not Used
D1 | ORN | 1340 | Fused Battery Feed
D2-D3 | -- | -- | Not Used
D4 | LT GRN | 275 | Transaxle Range Switch Feed-PARK
D5 | PNK | 1339 | Fused Ignition 1 Feed
D8-D10 | -- | -- | Not Used
D11 | TAN/BLK | 231 | Oil Pressure Switch Signal
D12 | -- | -- | Not Used
E1 | ORN | 1340 | Fused Battery Feed
E2-E4 | -- | -- | Not Used
E5 | YEL | 317 | Fog Lamp Relay Feed-Coil
E6 | -- | -- | Not Used
E7 | BLK | 28 | Horn Relay Output-Coil
E8 | DK GRN | 389/389 | Vehicle Speed Signal
E9-E10 | -- | -- | Not Used
E11 | LT GRN/BLK | 311/wT90 | High Beam Headlamp Feed-Right
E11 | YEL | 18 | Stop/Turnlamp Feed-Left Rear
E12 | -- | -- | Not Used
F1-F3 | -- | -- | Not Used
F4 | DK GRN/WHT | 711/wT90 | High Beam Headlamp Feed
F4 | LT GRN | 11 | High Beam Headlamp Feed
F5 | PPL | 34/34 | Fog Lamp Feed
F6 | -- | -- | Not Used
F7 | ORN | 640 | Fused Battery Feed
F8 | YEL | 712/wT90 | Low Beam Headlamp Feed
F8 | TAN | 12 | Low Beam Headlamp Feed
F9 | LT BLU | 14 | Turn Signal Lamp Feed-Left Front
F10 | DK BLU | 15 | Turn Signal Lamp Feed-Right Front
F11 | BRN | 9 | Park Lamp Feed
F12 | TAN/WHT | 312/wT90 | Low Beam Headlamp Feed
F12 | DK GRN | 19 | Stop/Turnlamp Feed-Right Rear

#### Junction Block C3 Underhood

Connector Part Information |

• | 15303507

• | 68-Way F Metri-pack 280 Series Flexlock (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A3 | -- | -- | Not Used
A4 | LT GRN | 11 | High Beam Headlamp Feed
A5 | PPL | 34 | Fog Lamp Feed
A6 | -- | -- | Not Used
A7 | DK GRN | 29 | Horn Feed
A8 | YEL | 712/wT90 | Low Beam Headlamp Feed
A8 | TAN | 12 | Low Beam Headlamp Feed
A9 | LT BLU | 14 | Turn Signal Lamp Feed-Left Front
A10 | DK BLU | 15 | Turn Signal Lamp Feed-Right Front
A11 | BRN | 9 | Park Lamp Feed
A12 | TAN/WHT | 312 | Low Beam Headlamp Feed-Right
A12 | DK GRN | 19 | Stop/Turnlamp Feed-Right Rear
B1-B3 | -- | -- | Not Used
B4 | LT GRN | 11 | High Beam Headlamp Feed
B5 | PPL | 34 | Fog Lamp Feed
B6 | -- | -- | Not Used
B7 | DK GRN | 29 | Horn Feed
B8 | TAN | 12 | Low Beam Headlamp Feed
B9-B10 | -- | -- | Not Used
B11 | BRN | 9 | Park Lamp Feed
B12 | -- | -- | Not Used
C1-C10 | -- | -- | Not Used
C11 | BRN | 9 | Park Lamp Feed
C12 | -- | -- | Not Used
D1-D10 | -- | -- | Not Used
D11 | BRN | 9 | Park Lamp Feed
D12 | -- | -- | Not Used
E1-E8 | -- | -- | Not Used
E9 | PNK | 339 | Ignition 1 Fused Output
E10 | -- | -- | Not Used
E11 | LT GRN/BLK | 311/wT90 | High Beam Headlight Feed
E11 | YEL | 18 | Stop/Turnlamp Feed-Left Rear
E12 | -- | -- | Not Used
F1-F12 | -- | -- | Not Used

#### Junction Block C4 Underhood

Connector Part Information |

• | 12146038

• | 2-Way F MaxiFuse (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 242 | Fused Battery Feed
B | RED | 142/142 | Fused Battery Feed

#### Junction Block C5 Underhood

Connector Part Information |

• | 12146037

• | 2-Way F MaxiFuse (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 42 | Fused Battery Feed

#### Junction Block C6 Underhood

Connector Part Information |

• | 12160605

• | 2-Way F MaxiFuse (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 642 | Fused Battery Feed
B | RED | 742 | Fused Battery Feed

#### Relay Block (Domestic)

Connector Part Information |

• | 12160504

• | 36-Way F Metri-pack 280 series Flex Lock (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A9 | -- | -- | Not Used
B1 | DK BLU | 75 | Accessory Relay Output
B2 | -- | -- | Not Used
B3 | ORN | 2240 | Battery Fused Output
B4 | -- | -- | Not Used
B5 | PPL | 293 | Rear Defogger Feed
B6 | -- | -- | Not Used
B7 | BRN | 241 | Ignition 3 Fused Output
B8 - B9 | -- | -- | Not Used
C1 | BLK | 707 | Accessory Relay Coil Feed
C2 | -- | -- | Not Used
C3 | RED | 142 | Battery Fused Output
C4 | -- | -- | Not Used
C5 | WHT | 193 | Rear Defogger Relay Coil Output
C6 | -- | -- | Not Used
C7 | ORN | 1040 | Battery Fused Output
C8 - C9 | -- | -- | Not Used
D1-D9 | -- | -- | Not Used

#### Relay Block (Export)

Connector Part Information |

• | 12160504

• | 36-Way F Metri-pack 280 series Flex Lock (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A9 | -- | -- | Not Used
B1 | ORN | 1640 | Battery Fused Output
B1 | DK BLU | 75 | Accessory Relay Output
B2 | -- | -- | Not Used
B3 | ORN | 1640 | Battery Fused Output
B3 | ORN | 2240 | Battery Fused Output
B4 | -- | -- | Not Used
B5 | PPL | 293 | Rear Defogger Feed
B6 | -- | -- | Not Used
B7 | BRN | 241 | Ignition 3 Fused
B8-B9 | -- | -- | Not Used
C1 | YEL | 1870 | Rear Fog Lamp Light Control Output
C1 | BLK | 707 | Accessory Relay Coil Feed
C2 | -- | -- | Not Used
C3 | RED | 122 | Rear Fog Lamp Feed
C3 | RED | 142 | Battery Fused Output
C4 | -- | -- | Not Used
C5 | WHT | 193 | Rear Defogger Relay Coil Output
C6 | -- | -- | Not Used
C7 | ORN | 1040 | Battery Fused Output
C8-C9 | -- | -- | Not Used
D1-D9 | -- | -- | Not Used