For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
3. Remove the license plate lamp sockets by turning the sockets counterclockwise.
4. Remove the liftgate handle nuts from the studs inside the liftgate.
5. Remove the bolts from the liftgate handle.
6. Remove the liftgate latch cable from the handle.
7. Remove the liftgate handle from the liftgate.

### Installation Procedure

1. Install the liftgate latch cable to the liftgate handle.
2. Align the liftgate handle studs with holes in liftgate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the liftgate handle retaining bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the liftgate handle retaining nuts to the studs.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

5. Install license plate lamp sockets by turning sockets clockwise.
6. Install the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
7. Close the liftgate.