For 1990-2009 cars

#### Tools Required

• | J 21854-01 Pivot Pin Remover

• | J 41688 Centering Sphere Installer Tool

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

1. Disable the inflatable restraint steering wheel module. Refer to Disabling the SIR System in SIR.
2. Remove the electronic lock module assembly. Refer to Electronic Column Lock Module - Disassemble - Off Vehicle .
3. Remove the tilt spring. Refer to Tilt Spring - Disassemble - Off Vehicle .
4. Remove the turn signal and multifunction switch assembly. Refer to Turn Signal and Multifunction Switch Assembly - Disassemble - Off Vehicle .
5. Remove the linear shift assembly. Refer to Linear Shift Assembly - Disassemble - Off Vehicle .
6. Remove the steering shaft seal (6).
7. Remove the sensor retainer (5).
8. Remove the lower spring retainer (4).
9. Remove the lower bearing spring (3).
10. Remove the lower bearing seat (2).
11. Remove the adapter and bearing assembly (1).
12. Remove the 2 pivot pins (3) from the steering column support assembly (1) using the tool J 21854-01 .
13. Remove the tilt head assembly (1) from the steering column jacket (2) with the lower steering shaft (3) still attached.
14. Remove the tilt head assembly (1) from the steering shaft assembly (2).

Important: Mark the upper shaft assembly and the lower steering shaft assembly to ensure proper assembly. Failure to assemble properly will cause the steering wheel to be turned 180 degrees.

15. Tilt the upper shaft assembly (1) 90 degrees to the lower steering shaft assembly (2) and disengage.
16. Insert the race and upper shaft assembly (1) into J 41688 .
17. Insert J 41688 into a vise.
18. Rotate the driver 90 degrees in the counterclockwise direction in order to disengage the centering sphere from the race and upper shaft assembly.
19. Remove the race and upper shaft assembly (1) from J 41688 .
20. Remove the shaft preload spring and the centering sphere fromJ 41688 .
21. If necessary, discard the old centering sphere and the old shaft preload spring.
22. Remove the 4 TORX® screws (2) from the steering column support assembly (1).