For 1990-2009 cars

### Removal Procedure

1. Remove the oil pan and the gasket. Refer to Oil Pan Replacement .
2. Remove the filter (100).
3. Remove the lip ring seal pressed into the case only if replacement is necessary.
4. Inspect the screen for the following foreign material:

• | Metal particles.

• | Clutch facing material.

• | Rubber particles.

• | Engine coolant.

5. Determine the source of the contamination if foreign material is evident. Repair as necessary.
6. Clean the screen and allow the screen to dry completely.

### Installation Procedure

1. If removed, install a new seal (101).
2. Install the filter (100).
3. Install the gasket and the oil pan. Refer to Oil Pan Replacement .