For 1990-2009 cars

#### Tool Required

J 36850 Assembly Lubricant (or equivalent)

1. Apply J 36850 or equivalent to a new turbine shaft O-ring seal (520).
2. Apply J 36850 or equivalent to the turbine shaft (518) splines.
3. Install the turbine shaft O-ring seal (520) onto the turbine shaft (518).

Caution: The torque converter weighs approximately 65 lbs. Personal injury may result if you lift the torque converter improperly.

4. Install the torque converter assembly (1).