For 1990-2009 cars

### Removal Procedure

1. Remove the overhead console. Refer to Roof Console Replacement in Interior Trim.
2. Disconnect the microphone electrical connector.
3. Remove the microphone from the headliner.

### Installation Procedure

1. Install the microphone to the headliner.
2. Connect the microphone electrical connector.
3. Install the overhead console. Refer to Roof Console Replacement in Interior Trim.