For 1990-2009 cars

### Removal Procedure

1. Use a flat-bladed tool to remove the plastic center cap from the center of the recliner handle.
2. Pull the recliner handle off the shaft.

### Installation Procedure

1. Install the recliner handle on the recliner shaft.
2. Push the recliner handle firmly onto the recliner shaft until fully seated.
3. Install the plastic center cap into the center of the recliner handle.