For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator to access the HVAC module. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connector to the temperature valve electric actuator.
3. Remove the mounting screws to the temperature valve electric actuator.
4. Remove the temperature valve electric actuator.

### Installation Procedure

1. Install the temperature valve electric actuator.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the mounting screws to the temperature valve electric actuator.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).

3. Connect the electrical connector to the temperature valve electric actuator.
4. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.