For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel upper trim. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Disengage the retaining tabs in order to remove the remote control door lock control receiver from the instrument panel upper trim.
3. Disconnect the remote control door lock receiver electrical connector.

### Installation Procedure

1. Connect the remote control door lock receiver electrical connector.
2. Engage the retaining tabs in order to install remote control door lock control receiver to the instrument panel upper trim.
3. Install the instrument panel upper trim. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gauges and Console.