For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls -- 3.4L.
2. Use a hammer and a chisel in order to raise the transaxle vent seat off of the transaxle (37).
3. Use a flat-bladed tool in order to pry the transaxle vent out of the transaxle (37).

### Installation Procedure

1. Use a small hammer and a flat-bladed tool and tap down on the transaxle vent seat in order to install the transaxle vent (37).
2. Install the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls -- 3.4L.