For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Modulator Bleeder Valves | 9 N·m | 80 lb in
Brake Caliper Bleeder Valve (Front) | 13N·m | 115 lb in
Brake Caliper Bleeder Valve (Rear) | 11N·m | 97 lb in
Brake Pedal Maximum Travel * | 74 mm | 2.91 in
Brake Rear Wheel Cylinder Bleeder Valve | 7N·m | 62 lb in
Brake System Flushing

- Brake Fluid Volume from the ABS Modulator Bleeder Valves

118 ml

4 oz

- Brake Fluid Volume from the TCS Modulator Bleeder Valves

118 ml

4 oz

- Brake Fluid Volume from the Brake Calipers

235 ml

8 oz

Brake System Pressure Bleed

- Initial Pressure Adjustment Setting (Leak Testing the Hydraulic Brake System)

70 kPa

10 psi

- Pressure Bleed Procedure Setting

240 kPa

35 psi

TCS Modulator Bleeder Valves | 9 N·m | 80 lb in
Proportioning Valve Cap | 27 N·m | 20 lb ft
* Specification with 450 N (100 lbs) of force applied to the brake pedal, the ignition OFF and the brake booster vacuum depleted.