For 1990-2009 cars

### Removal Procedure

1. Lower the front door window.
2. Remove the outside rearview mirror. Refer to Power Mirror Replacement .
3. Use a flat-bladed tool in order to pry up at the front of the outer belt sealing strip from the inside edge.
4. Remove the front door outer belt window sealing strip from the pinch-weld flange.

### Installation Procedure

1. Install the front door outer belt window sealing strip to the pinch-weld flange.
2. Use hand pressure in order to firmly seat the outer belt sealing strip.
3. Install the outside rearview mirror. Refer to Outside Rearview Mirror Motor Replacement .
4. Raise the front door window.