For 1990-2009 cars

### Removal Procedure

1. Loosen/remove the wheel nut caps.
2. Use a flat-bladed tool in order to pry the edge of the wheel cover out.
3. Use your fingers in order to pull the wheel cover off of the wheel.
4. Place the wheel cover down with the finished surface facing up. Do Not place anything on top of the wheel cover.

### Installation Procedure

1. Install the wheel cover.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the wheel nut caps.

Tighten
Tighten the wheel nut caps to 3 N·m (27 lb in).