For 1990-2009 cars

### Removal Procedure

1. Use a small flat-bladed tool in order to remove the nozzle (2) from the liftgate.
2. Remove the washer hose (1) from the nozzle (2).

### Installation Procedure

1. Install the washer hose (1) to the nozzle (2).
2. Perform the following steps in order to install the nozzle (2) to the liftgate:

2.1. | Align the nozzle (2) to the hole.

2.2. | Push in the nozzle (2).