For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls -- 3.4L.
2. Use a flat-bladed tool in order to remove the retaining clip from the automatic transaxle range selector cable.
3. Use a large flat-bladed tool in order to remove the automatic transaxle range selector cable from the cable lever.
4. Use pliers in order to depress the cable retainers.
5. Remove the automatic transaxle range selector cable from the automatic transaxle range selector cable bracket.
6. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.
7. Remove the retaining clip from the automatic transaxle range selector cable.
8. Remove the automatic transaxle range selector cable from the column control lever.
9. Remove the automatic transaxle range selector cable from the steering column bracket.
10. Remove the automatic transaxle range selector cable through the hole in the cowl.

### Installation Procedure

1. Properly route the automatic transaxle range selector cable through the engine compartment.
2. Install the automatic transaxle range selector cable through the cowl.
3. Install the automatic transaxle range selector cable to the steering column bracket.
4. Install the retaining clip to the automatic transaxle range selector cable.
5. Install the automatic transaxle range selector cable to the column control lever.
6. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.
7. Install the automatic transaxle range selector cable to the automatic transaxle range selector cable bracket.
8. Install the automatic transaxle range selector cable to the automatic transaxle range selector lever.
9. Install the retaining clip to the automatic transaxle range selector cable.
10. Adjust the automatic transaxle range selector cable. Refer to Range Selector Lever Cable Adjustment .
11. Install the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls -- 3.4L.