For 1990-2009 cars

### Removal Procedure

Caution: An electric fan under the hood can start up even when the engine is not running and can injure you. Keep hands, clothing and tools away from any underhood electric fan.

Caution: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

Important: If abnormal noise or vibration is felt from the engine compartment, inspect and clean any foreign material from the cooling fan blades.

1. Turn the ignition off.
2. Remove the cooling fans with the cooling fan shroud. Refer to Engine Cooling Fan Replacement .
3. Remove the cooling fans. Refer to Fan Replacement .
4. Remove the cooling fan motors from the cooling fan shroud. Refer to Engine Coolant Fan Motor Replacement .
5. Remove the cooling fan motor heat shields from the cooling fan shroud.

### Installation Procedure

1. Install the cooling fan motor heat shields to the cooling fan shroud.
2. Install the cooling fan motors to the cooling fan shroud. Refer to Engine Coolant Fan Motor Replacement .
3. Install the cooling fans. Refer to Fan Replacement .
4. Install the cooling fans with the cooling fan shroud. Refer to Engine Cooling Fan Replacement .