For 1990-2009 cars

#### Tools Required

J 41131 Engine Tilt Strap

1. Remove the throttle body air inlet duct. Refer to Air Filter Element Replacement in Engine Controls - 3.4L.
2. Set the park brake.
3. Shift the transaxle into Neutral.
4. Remove the engine mount strut bolts. Swing the engine mount struts aside. Refer to Engine Mount Strut Replacement and Engine Mount Strut Replacement .
5. Install the J 41131 .
6. Pull on the engine in order to rotate the engine forward.
7. Tighten the J 41131 .