For 1990-2009 cars

#### Tools Required

J 42506 Door Handle Clip Remover

### Removal Procedure

1. Use J 42506 in order to remove the inside door handle clip.
2. Remove the inside handle from the sliding door.

### Installation Procedure

1. Load the clip into the inside door handle with the open end facing up.
2. Align the handle with the shaft on the sliding door.
3. Press firmly in order to seat the inside handle to the sliding door.