For 1990-2009 cars

### Removal Procedure

Notice: When you are servicing the automatic level control sensor link, ensure that the sensor link and the sensor arm are not damaged. Ensure the sensor arm and the sensor link are properly oriented. Improper orientation of the sensor arm and the sensor link may cause damage to the automatic level control system or the vehicle.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the ALC sensor link from the tie rod ball stud. Remove the ALC sensor link from the sensor arm ball stud.

### Installation Procedure

1. Install the link to the tie rod and the sensor arm.
2. Lower the vehicle.