For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: The SECURITY indicator is on or (flashing) at all times or is inoperative
1 | Did you perform the theft deterrent diagnostic system check? | -- | Go to Step 2 | Go to Diagnostic System Check - Theft Deterrent
2 |

1. Turn ON the ignition, with the engine OFF.
2. Observe the battery indicator telltale on the reconfiguralbe diplay.

Does the battery indicator turn on during bulb check?

--

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 3

3 | Replace the IPC. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges, and Console. Important: Perform the set up procedure for the IP. Did you complete the replacement and the set up procedure? | -- | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2