For 1990-2009 cars

#### Diagnostic Trouble Codes (DTC) List/Type

Description | Domestic RPO LA1 | Export Unleaded Fuel | Export Leaded Fuel
--- | --- | --- | ---
DTC P0101 Mass Air Flow (MAF) Sensor Performance | B | B | --
DTC P0102 Mass Air Flow (MAF) Sensor Circuit Low Frequency | B | B | --
DTC P0103 Mass Air Flow (MAF) Sensor Circuit High Frequency | B | B | --
DTC P0107 Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | B | B | --
DTC P0108 Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | B | B | --
DTC P0112 Intake Air Temperature (IAT) Sensor Circuit Low Voltage | B | B | --
DTC P0113 Intake Air Temperature (IAT) Sensor Circuit High Voltage | B | B | --
DTC P0117 Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | B | B | --
DTC P0118 Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | B | B | --
DTC P0121 Throttle Position (TP) Sensor Performance | B | B | --
DTC P0122 Throttle Position (TP) Sensor Circuit Low Voltage | B | B | --
DTC P0123 Throttle Position (TP) Sensor Circuit High Voltage | B | B | --
DTC P0125 Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | B | B | --
DTC P0131 HO2S Circuit Low Voltage Sensor 1 | B | B | --
DTC P0132 HO2S Circuit High Voltage Sensor 1 | B | B | --
DTC P0133 HO2S Slow Response Sensor 1 | B | B | --
DTC P0134 HO2S Circuit Insufficient Activity Sensor 1 | B | B | --
DTC P0135 HO2S Heater Performance Sensor 1 | B | B | --
DTC P0137 HO2S Circuit Low Voltage Sensor 2 | B | B | --
DTC P0138 HO2S Circuit High Voltage Sensor 2 | B | B | --
DTC P0140 HO2S Circuit Insufficient Activity Sensor 2 | B | B | --
DTC P0141 HO2S Heater Performance Sensor 2 | B | B | --
DTC P0171 Fuel Trim System Lean | B | B | --
DTC P0172 Fuel Trim System Rich | B | B | --
DTC P0201 Injector 1 Control Circuit | B | B | --
DTC P0202 Injector 2 Control Circuit | B | B | --
DTC P0203 Injector 3 Control Circuit | B | B | --
DTC P0204 Injector 4 Control Circuit | B | B | --
DTC P0205 Injector 5 Control Circuit | B | B | --
DTC P0206 Injector 6 Control Circuit | B | B | --
DTC P0218 Transmission Fluid Overtemperature in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0230 Fuel Pump Relay Control Circuit | C | C | --
DTC P0300 Engine Misfire Detected | B | B | --
DTC P0325 Knock Sensor (KS) Circuit | B | B | --
DTC P0327 Knock Sensor (KS) Circuit | B | B | --
DTC P0336 Crankshaft Position (CKP) Sensor Performance | B | B | --
DTC P0341 Camshaft Position (CMP) Sensor Performance | B | B | --
DTC P0401 Exhaust Gas Recirculation (EGR) Flow Insufficient | A | A | --
DTC P0403 Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | B | B | --
DTC P0404 Exhaust Gas Recirculation (EGR) Open Position Performance | B | B | --
DTC P0405 Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | B | B | --
DTC P0410 Secondary Air Injection (AIR) System | B | B | --
DTC P0412 Secondary Air Injection (AIR) Solenoid Control Circuit | B | B | --
DTC P0418 Secondary Air Injection (AIR) Pump Relay Control Circuit | B | B | --
DTC P0420 Catalyst System Low Efficiency | A | A | --
DTC P0440 Evaporative Emission (EVAP) System | B | B | --
DTC P0442 Evaporative Emission (EVAP) System Small Leak Detected | A | A | --
DTC P0443 Evaporative Emission (EVAP) Purge Solenoid Control Circuit | B | B | --
DTC P0446 Evaporative Emission (EVAP) Vent System Performance | B | B | --
DTC P0449 Evaporative Emission (EVAP) Vent Solenoid Control Circuit | B | B | --
DTC P0452 Fuel Tank Pressure Sensor Circuit Low Voltage | B | B | --
DTC P0453 Fuel Tank Pressure Sensor Circuit High Voltage | B | B | --
DTC P0462 Fuel Level Sensor Circuit Low Voltage | C | C | --
DTC P0463 Fuel Level Sensor Circuit High Voltage | C | C | --
DTC P0480 Cooling Fan Relay 1 Control Circuit | B | B | --
DTC P0481Cooling Fan Relay 2 Control Circuit | B | B | --
DTC P0502 Vehicle Speed Sensor (VSS) Circuit Low Input in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0503 Vehicle Speed Sensor (VSS) Circuit Intermittent in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0506 Idle Speed Low | B | B | --
DTC P0507 Idle Speed High | B | B | --
DTC P0530 Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit | C | C | --
DTC P0560 System Voltage | C | C | --
DTC P0601 Control Module Read Only Memory (ROM) | A | A | --
DTC P0602 Control Module Not Programmed | A | A | --
DTC P0620 Generator Performance | C | C | --
DTC P0650 Malfunction Indicator Lamp (MIL) Control Circuit | B | B | --
DTC P0711 TFT Sensor Circuit Range/Performance in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0712 Transmission Fluid Temperature (TFT) Sensor Circuit Low Input in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0713 Transmission Fluid Temperature (TFT) Sensor Circuit High Input in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0716 Input Speed Sensor Circuit Intermittent in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0717 Input Speed Sensor Circuit Low Input in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0719 Brake Switch Circuit Low Input in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0724 Brake Switch Circuit High Input in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0730 Incorrect Gear Ratio in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0741 TCC System Stuck Off in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0742 TCC System Stuck On in Automatic Transaxle - 4T65 - E | B | A | --
DTC P0748 Pressure Control Solenoid Circuit Electrical in Automatic Transaxle - 4T65 - E | C | C | --
DTC P0751 1-2 Shift Solenoid Valve Performance - No First or Fourth Gear in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0752 1-2 Shift Solenoid Valve Performance - No Second or Third Gear in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0753 1-2 Shift Solenoid Circuit Electrical in Automatic Transaxle - 4T65 - E | B | B | --
DTC P0756 2-3 Shift Solenoid Valve Performance - No First or Second Gear in Automatic Transaxle - 4T65 - E | A | A | --
DTC P0757 2-3 Shift Solenoid Valve Performance - No Third or Fourth Gear in Automatic Transaxle - 4T65 - E | A | A | --
DTC P0758 2-3 Shift Solenoid Circuit Electrical in Automatic Transaxle - 4T65 - E | A | A | --
DTC P1106 Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | C | C | --
DTC P1107 Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | C | C | --
DTC P1111 Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | C | C | --
DTC P1112 Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage | C | C | --
DTC P1114 Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | C | C | --
DTC P1115 Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | C | C | --
DTC P1121 Throttle Position (TP) Sensor Circuit Intermittent High Voltage | C | C | --
DTC P1122 Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | C | C | --
DTC P1133 HO2S Insufficient Switching Sensor 1 | B | B | --
DTC P1134 HO2S Transition Time Ratio Sensor 1 | B | B | --
DTC P1336 Crankshaft Position (CKP) System Variation Not Learned | A | A | --
DTC P1351 Ignition Coil Control Circuit High Voltage | B | B | --
DTC P1352 Ignition Bypass Circuit High Voltage | B | B | --
DTC P1361 Ignition Control (IC) Circuit Low Voltage | B | B | --
DTC P1362 Ignition Bypass Circuit Low Voltage | B | B | --
DTC P1374 Crankshaft Position (CKP) High to Low Resolution Frequency Correlation | B | B | --
DTC P1380 Misfire Detected - Rough Road Data Not Available | C | C | --
DTC P1381 Misfire Detected - No Communication with Brake Control Module | C | C | --
DTC P1404 Exhaust Gas Recirculation (EGR) Closed Position Performance | A | A | --
DTC P1441 Evaporative Emission (EVAP) System Flow During Non-Purge | B | B | --
DTC P1483 Engine Cooling System Performance | C | C | --
DTC P1546 Air Conditioning (A/C) Clutch Relay Control Circuit | C | C | --
DTC P1554 Cruise Control Feedback Circuit | C | C | --
DTC P1571 Traction Control Torque Request Circuit | C | C | --
DTC P1585 Cruise Control Inhibit Output Circuit | C | C | --
DTC P1626 Theft Deterrent Fuel Enable Signal Lost | C | C | --
DTC P1630 Theft Deterrent Learn Mode Active | C | C | --
DTC P1631 Theft Deterrent Start Enable Signal Not Correct | C | C | --
DTC P1635 5 Volt Reference Circuit | B | B | --
DTC P1639 5 Volt Reference 2 Circuit | C | B | --
DTC P1689 Traction Control Delivered Torque Output Circuit | C | C | --
DTC P1810 TFP Valve Position Switch Circuit in Automatic Transaxle - 4T65 - E | B | B | --
DTC P1811 Maximum Adapt and Long Shift in Automatic Transaxle - 4T65 - E | C | C | --
DTC P1814 Torque Converter Overstressed in Automatic Transaxle - 4T65 - E | C | C | --
DTC P1860 TCC PWM Solenoid Circuit Electrical in Automatic Transaxle - 4T65 - E | A | B | --
DTC P1887 TCC Release Switch Circuit in Automatic Transaxle - 4T65 - E | B | B | --
U1000 Class II Communication Malfunction Refer to DTC U1000 and DTC U1255 Class 2 Communication Malfunction in Data Link Communications. | -- | -- | --
U1016 Class II Lost Communication with PCM Refer to DTC U1001-U1254 Lost Communication with XXX in Data Link Communications. | -- | -- | --
U1255 Class II Communication Malfunction Refer to DTC U1000 and DTC U1255 Class 2 Communication Malfunction in Data Link Communications. | -- | -- | --
U1300 Class II Data Link Low Refer to DTC U1300 Class 2 Data Link Low in Data Link Communications. | -- | -- | --
U1301 Class II Data Link High Refer to DTC U1301 Class 2 Data Link High in Data Link Communications. | -- | -- | --
U1305 Class II Data Link Low or High Refer to DTC U1305 Class 2 Data Link Low or High in Data Link Communications. | -- | -- | --