For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Peel the water deflector from the inner door.

### Installation Procedure

Important: Ensure proper adhesive bonding of the sliding door water deflector to the inner panel. Proper adhesive bonding helps to prevent water leaks.

1. Position the water deflector to the door.
2. Press the water deflector onto the inner door.
3. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .