For 1990-2009 cars

### Removal Procedure

1. Remove the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
2. Remove the seat back pad from the frame (1).
3. Squeeze the bottom of the head restraint guide together and pull the head restraint guide from the seat back frame.
4. Remove the seat back frame (1).

### Installation Procedure

1. Install the seat back frame (1).
2. Push the head restraint guide into the seat back frame. Make sure it locks into place.
3. Install the seat back pad to the frame (1).
4. Install the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .