For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Auxiliary Coolant Bypass Pump | Engine Compartment above the air cleaner assembly secured to the diagonal brace bracket | Cooling System Component Views | Cooling System Connector End Views
Auxiliary Coolant Pump Switch | Body front, inside center front bumper beam | Cooling System Component Views | Cooling System Connector End Views
Engine Coolant Fan Motor 1 (RH) | Mounted to the rear left side of the radiator | Cooling System Component Views | Cooling System Connector End Views
Engine Coolant Fan Motor 2 (LH) | Mounted to the rear right side of the radiator | Cooling System Component Views | Cooling System Connector End Views
Engine Coolant Level Indicator Module | Mounted to the rear right side of the radiator, below the radiator cap | Cooling System Component Views | Cooling System Connector End Views
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C105 (4 cavities) | Engine wiring harness to the engine coolant fan wiring harness, behind the engine coolant fan 1 (left) | -- | Inline Harness Connector End Views
G117 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views | --
S105 | Engine harness, top right side radiator approximately 20 cm (8 in) from the engine coolant fan 1 (right) motor breakout | -- | --