For 1990-2009 cars

### Removal Procedure

The fuel pump relay is mounted in the right front corner of the engine compartment.

1. Turn OFF the ignition.
2. Remove the fuel pump relay retaining bolt.
3. Disconnect the fuel pump relay electrical connector.
4. Remove the relay from the vehicle.

### Installation Procedure

1. Connect the fuel pump relay electrical connector.
2. Position the fuel pump relay on the radiator core support.
3. Install the fuel pump relay retaining screw through the relay into the radiator core support.