For 1990-2009 cars

### Removal Procedure

1. Remove the left side insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Remove the booster push rod (2) from the brake pedal (1).
3. Disconnect the electrical connectors from the cruise control release and stoplamp switches.
4. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
5. Disable the SIR system. Refer to Disabling the SIR System in SIR.
6. Remove the brake booster mounting nuts (3).
7. Remove the brake pedal bracket mounting nuts (2).
8. Remove the upper mounting bolt from the brake pedal brace (4).
9. Remove the brake pedal with the bracket (3).
10. Remove the brake pedal brace (4) from the bracket.
11. Remove the cruise control release switch (3) and the stoplamp switch (1) from the brake pedal with the bracket (2).

### Installation Procedure

1. Install the cruise control release switch (3) and the stoplamp switch (1) to the brake pedal with the bracket (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the brake pedal brace (4) with the mounting nuts (1) to the bracket.

Tighten
Tighten the nuts (1) to 10 N·m (89 lb in).

3. Install the brake pedal with the bracket (3).
4. Install the upper mounting bolt for the brake pedal brace (4).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

5. Install the brake pedal bracket mounting nuts (2).

Tighten
Tighten the nuts (2) to 25 N·m (18 lb ft).

6. Install the brake booster mounting nuts (3).

Tighten
Tighten the nuts (3) to 25 N·m (18 lb ft).

7. Enable the SIR system. Refer to Enabling the SIR System in SIR.
8. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
9. Connect the electrical connectors to the cruise control release and stoplamp switches.
10. Install the booster push rod (2) to the brake pedal (1).
11. Adjust the stoplamp switch and the cruise control release switch. Refer to Stop Lamp Switch Adjustment .
12. Install the left side insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.