For 1990-2009 cars

### Removal Procedure

1. Remove the rear seats. Refer to Rear Seat Replacement .
2. Remove the locking clips from the bezel using a curved pick tool.
3. Remove the anchor plate bezel (1) from the floor.

### Installation Procedure

1. Press into place the anchor plate bezel (1) to the floor.
2. Press into place the locking clips to the bezel.
3. Install the rear seats. Refer to Rear Seat Replacement .