For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control Systems | Body Control System Connector End Views in Body Control Systems
Front Door Lock | Inside, rear end of the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Lock (Ajar Indicator Switch) | Part of the front door lock | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | -- | --
Ignition Key Alarm Switch | Part of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Guages and Console | --
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Guages and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Guages and Console
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | -- | --
Turn Signal and Headlamp Dimmer Switch and Windshield Wiper and Windshield Washer Switch | Inside the steering column | -- | --
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | -- | --
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | -- | --
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | -- | --
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | -- | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G302 | Secured near the base of the right B-pillar | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | -- | --
P500 | Between the left A-pillar and the left front door | -- | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S232 | IP harness, right side of the IP approximately 17 cm (7 in) from the radio breakout | -- | --
S233 | IP harness, left side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --