For 1990-2009 cars

### Removal Procedure

1. Open the compartment door.
2. Pry the compartment lamp outward in order to remove the compartment lamp.
3. Remove the bulb from the socket.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the bulb into the lamp socket.
3. Apply pressure to the compartment lamp until the compartment lamp snaps in.
4. Close the compartment door.