For 1990-2009 cars

## Compressor Pressure Relief Valve Installation V5 - Direct Mount

#### Tool Required

J 41790-A Compressor Holding Fixture

1. Clean the pressure relief valve seat area of the rear head.
2. Lubricate the O-ring of the new pressure relief valve with clean 525 viscosity refrigerant oil.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the new pressure relief valve into the compressor.

Tighten
Tighten the pressure relief valve to 9 N·m (80 lb in).

4. Remove the compressor from the J 41790-A .