For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .
3. Remove the steering wheel. Refer to Steering Wheel Replacement in Steering Wheel and Column-Tilt.
4. Remove the upper and lower steering column shrouds.
5. Disconnect the radio steering wheel controls inline connector C205 located at the base of the steering column.
6. Remove the wiring harness straps from the steering wheel column wiring harness.
7. Remove the retaining ring.
8. Remove the inflatable restraint steering wheel module coil from the steering shaft.

### Installation Procedure

1. Install the inflatable restraint steering wheel module coil to the steering shaft.
2. Install the retaining ring.
3. Route the lower coil wiring harness along steering column and install the necessary wiring harness straps.
4. Connect the radio steering wheel controls inline connector C205.
5. Install the upper and lower steering column shrouds.
6. Install the steering wheel. Refer to Steering Wheel Replacement in Steering Wheel and Column-Tilt.
7. Install the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .
8. Enable the SIR system. Refer to Enabling the SIR System .