For 1990-2009 cars

## Air Conditioning Clutch Coil Installation V5 - Direct Mount

#### Tools Required

• | J 33024 Clutch Coil Installer Adapter

• | J 33025 Clutch Coil Puller Legs

• | J 8433 Compressor Pulley Puller

• | J 8433-3 Forcing Screw

• | J 41790-A Compressor Holding Fixture

• | J 42136 A/C Lip Seal Remover

1. Place the clutch coil assembly (1) on the front head with the clutch coil terminal at the positioned at the mark made during disassembly.
2. Place the J 33024 over the internal opening of the clutch coil housing and align installer with the compressor front head.
3. Install the J 8433-3 into the J 8433 and center the screw in the countersunk center hole of the J 33024 .
4. Install the 4 inch through bolts and washers from the J 42136 tool kit into the J 33025 and attach them to the compressor mounting bosses.
5. Turn the center forcing screw of the J 8433 to press the clutch coil onto the front head until the clutch coil is fully seated.

Make sure the clutch coil and the J 33024 stay in-line with each other while pressing the clutch coil onto the compressor.

6. Install the compressor clutch rotor and bearing assembly. Refer to Clutch Rotor and/or Bearing Install .
7. Install the compressor clutch plate and hub assembly. Refer to Compressor Clutch Plate/Hub Assembly Install .
8. Remove the compressor from the J 41790-A .