For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Remove the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the powersliding door unlatch release actuator electrical connector.
4. Remove the powersliding door unlatch release actuator screws.
5. Remove the powersliding door unlatch release actuator from the powersliding door.
6. Unhook the powersliding door latch release actuator rod from the powersliding door latch release actuator.

### Installation Procedure

1. Hook the powersliding door latch release actuator rod to the powersliding door latch release actuator.
2. Install the powersliding door unlatch release actuator to the powersliding door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the powersliding door unlatch release actuator screws.

Tighten
Tighten the powersliding door unlatch release actuator screws to 10 N·m (89 lb in).

4. Connect the powersliding door unlatch release actuator electrical connector.
5. Install the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
6. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
7. Perform the reinitialization procedure. Refer to Power Sliding Door (PSD) Re-Initialization .