For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Driver Information Display | In the roof console | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Electronic Brake Control Module (EBCM) | Lower left side of the engine compartment | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Below the right front seat | SIR Component Views | SIR Connector End Views
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Pass Key III Module | In the steering column, at the ignition switch | -- | Theft Deterrent System Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Radio | Center of the IP console | Entertainment Component Views | Entertainment Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S238 | IP harness, center of the IP approximately 80 cm (31 in) from the cigar lighter connector | -- | --