For 1990-2009 cars

#### Locked up in Drive/Reverse

Checks | Cause
--- | ---
DEFINITION: The vehicle cannot be moved forward or backward during the following conditions:

• | The engine is running.

• | The transmission is in Drive or Reverse range.

• | The vehicle brakes are not applied.

• | The throttle is closed (idling).

Manual Linkage | Misadjusted
Input and Reaction Carrier Assemblies | The input carrier assembly (672) or the reaction carrier assembly (675) components are damaged.
Differential Carrier Assembly |

• | The park pawl assembly (694) is broken or damaged.

• | The sun gear shaft (689), the internal gear assembly (693), or the carrier assembly (700) components are damaged.