For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Using J 38778 remove the upper seat belt anchor bolt from the belt guide loop.

Important: Use care to not break the locating tabs on the quarter trim when removing the back body pillar trim.

2. Remove the back body pillar trim from the vehicle.

### Installation Procedure

1. Install the back body pillar trim by aligning the trim with the locating tabs on the quarter trim.
2. Align the retainers in the holes and push to secure the retainers.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper seat belt anchor bolt to the belt guide loop.

Tighten
Tighten the bolt to 43 N·m (32 lb ft).