For 1990-2009 cars

### Removal Procedure

Caution: An electric fan under the hood can start up even when the engine is not running and can injure you. Keep hands, clothing and tools away from any underhood electric fan.

Caution: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

Important: If abnormal noise or vibration is felt from the engine compartment, inspect and clean any foreign material from the cooling fan blades.

1. Turn the ignition off.
2. Remove the cooling fans with the cooling fan shroud. Refer to Engine Cooling Fan Replacement .
3. Remove the cooling fan. Refer to Fan Replacement .
4. Remove the cooling fan motor electrical connector.
5. Remove the cooling fan motor screws.
6. Remove the cooling fan motor.

### Installation Procedure

1. Install the cooling fan motor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the cooling fan motor screws.

Tighten
Tighten the screws to 6 N·m (53 lb in).

3. Install the cooling fan motor electrical connector.
4. Install the cooling fan. Refer to Fan Replacement .
5. Install the cooling fans with the cooling fan shroud. Refer to Engine Cooling Fan Replacement .