For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
2. Remove the seat cushion frame from the seat cushion pad.
3. Remove the seat cushion support from the frame.

### Installation Procedure

1. Fasten the seat cushion support to the frame.
2. Install the seat cushion frame to the seat cushion pad.
3. Install the seat cushion cover. Refer to Front Seat Cushion Cover Replacement .