For 1990-2009 cars

## Rear Brake Rotor Replacement Export

### Removal Procedure

#### Tools Required

J 42450-A Hub Cleaning Kit

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the brake caliper bracket with the brake caliper.

Notice: Do not allow calipers to hang from the flexible hoses. Doing so can damage the hoses.

4. Use a strap or heavy gage wire in order to support the brake caliper and the brake caliper bracket.
5. Remove the brake rotor.

### Installation Procedure

1. Clean any corrosion from the brake rotor flange.
2. Use the J 42450-A in order to clean the hub flange.
3. Install the brake rotor.
4. Install the brake caliper bracket with the brake caliper. Refer to Rear Brake Caliper Replacement .
5. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
6. Lower the vehicle.