For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
2. Remove the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle in Steering Wheel and Column-Tilt.
3. Remove the upper steering column shroud.
4. Disconnect the electrical connector at the base of the steering column
5. Pull the PASS-Key III® module from the ignition lock cylinder housing.
6. Remove the electrical connector and wires from the steering column.
7. Remove the PASS-Key III® module from the vehicle.

### Installation Procedure

1. Install the PASS-Key III® module to the vehicle.
2. Install the electrical connector and wires to the column.
3. Slide the PASS-Key III® module over the ignition lock cylinder housing.
4. Connect the electrical connector at the base to the steering column.
5. Install the upper column shroud.
6. Install the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle in Steering Wheel and Column-Tilt.
7. Install the instrument panel knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.