For 1990-2009 cars

### Removal Procedure

1. Carefully release the locking tabs using a flat-bladed tool in the locations as indicated.
2. Remove the auxiliary video module from the overhead entertainment console.
3. Disconnect the electrical connectors from the auxiliary video module.

### Installation Procedure

1. Connect the electrical connectors to the auxiliary video module.
2. Install the auxiliary video module to the overhead entertainment console.
3. Press the auxiliary video module until it locks into place.