For 1990-2009 cars

#### Tools Required

J 41352 Modular Column Holding Fixture

1. Place the bottom of J 41352 into a vise.
2. Set the steering column in the J 41352 .
3. Place the top piece of J 41352 onto the column.
4. Pull the tilt lever out from the lower trim cover.
5. Remove the 2 pan head tapping screws (2) from the lower trim cover (1).
6. Remove the lower trim cover (1).
7. Remove the TORX® head screw (1) from the upper trim cover (2).
8. Slide the shift lever seal up the shift lever.
9. Remove the upper trim cover (2).
10. Remove the trim cover protector (1) from the lower trim cover (2).