For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip and/or Garnish Trim Clip Remover

### Removal Procedure

1. Remove the video entertainment system overhead console. Refer to VES Overhead Console Replacement .
2. Use the J 38778 in order to remove the interface module from the support bracket.
3. Disconnect the interface module electrical connectors from the interface module (2).

### Installation Procedure

1. Connect the electrical connectors to the interface module (2).
2. Using both hands, hold the interface module in a position where the hook and loop retainers are lined up with one another.
3. Secure the hook and loop retainer by working the interface module in a back and forth motion.
4. Install the video entertainment system overhead console. Refer to VES Overhead Console Replacement .