For 1990-2009 cars

### Removal Procedure

1. Remove the cushion pad from the frame. Refer to the appropriate sections in Rear Seat Cushion Pad Replacement , if equipped:

• | 60/40 split bench seat

• | Captain's chair

• | Rear bucket

• | 50/50 split bench seat

2. Remove the cushion support from the frame.

### Installation Procedure

1. Install the cushion support to the frame.
2. Install the cushion pad to the frame. Refer to the appropriate sections in Rear Seat Cushion Pad Replacement , if equipped:

• | 60/40 split bench seat

• | Captain's chair

• | Rear bucket

• | 50/50 split bench seat