For 1990-2009 cars

Important: The electrical contact on the turn signal and multifunction switch assembly must rest on the turn signal cancel cam assembly.

1. Install the turn signal and multifunction switch assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 2 pan head tapping screws.

Tighten
Tighten the screws to 7 N·m (62 lb in).

3. Slide the 2 connectors (2) of the turn signal and multifunction switch assembly onto the bulk head connector (1).
4. Install the wire harness assembly (4) into the wire harness strap (5).
5. Install the wire harness strap (2) into the steering column tilt head assembly (1).
6. Install the wire harness straps (3) onto the wire harness assembly (4).
7. Install the upper and lower trim covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .